C5GG25F1 - 206

REMOVAL - REFITTING FRONT SEAT

1 - REMOVAL

Push the seat fully forwards .

Remove the fasteners (1) - (2) .

Push the seat fully rearwards .

Remove the fasteners (3) - (4) .

SIDE AIRBAG

Disconnect the connectors under the seat .

ALL MODELS

Remove the seat .

2 - REFITTING

Refit the seat .

SIDE AIRBAG

Connect the connectors under the seat .

ALL MODELS

Refit the bolts (4) - (3) - (1) - (2) .

IMPERATIVE : observe the order of tightening shown .

G : Left front seat .

D : Right front seat .

Tightening torque(s) : 2,5 ± 0,3 da.Nm .

3 DOOR SALOON CABRIOLET

IMPERATIVE : slide the seat towards the front by using the cross piece and not the handle for access to the rear seats .