C5DG0NF1 - 206 CABRIOLET

REMOVAL - REFITTING DOOR ELECTRIC WINDOW MECHANISM

1 - TOOLS TO BE MADE LOCALLY

[1] Bolt (TH M10 x 21 mm) .

2 - REMOVAL

Remove :

- THE MIRROR CHEATER
- THE DOOR TRIM PANEL
- the sealing sheet
- the interior wipe seal
- THE EXTERNAL WEATHERSTRIP ON THE WINDOW
- THE DOOR WINDOW

Remove :

- the upper fixings (1)
- the closers and mountings

Disconnect the electric window motor connector (3) .

Detach the mechanism via the front opening .

Remove the window mechanism .

3 - REFITTING

Fit :

- the electric window mechanism in the box section
- the fixings (2) - (1) (without locking )

Adjust the window mechanism :

- place the front rail at the stop on the interior panel
- tighten the front lower mounting (2) to 0.7 ± 0.1 dan.m
- support the tool [1] on the interior panel to adjust the rear guide rail
- tighten the rear lower mounting (2) to 0.7 ± 0.1 dan.m

Tighten the fasteners (1) to 0.7 ± 0.1 da.Nm .

Refit the blanks .

Connect the electric window motor connector (3) .

REFIT THE DOOR WINDOW .

ADJUST THE WINDOW .

Proceed in the reverse order to removal .

IMPERATIVE : fit new seals, which must be assembled without folds and tears ; absolute cleanness of the contact face on the vehicle is necessary ; run a wheel over the parts of the flange to be bonded ; these recommendations are essential to prevent possible entry of water, dust or noise .

Test operation .