C5IG20F1 - 206 CABRIOLET

REMOVAL - REFITTING ROOF STRIKER SWITCHES

1 - REMOVAL

OPEN THE ROOF MANUALLY .

Remove :

- THE WINDSCREEN APERTURE UPPER FINISHER
- THE SCREEN PILLAR TRIM PADS
- THE ROOF STRIKERS

Push the centring devices (1) using a screwdriver .

Detach the adhesive (2) between the striker and the switch (3) using a screwdriver .

Remove the switch (3) .

2 - REFITTING

WARNING : do not press the metal blade of the switch .

Refit the switch (3) .

Fit the (1) correctly and apply pressure to the adhesive (2) .

REFIT THE ROOF STRIKER .

Test operation .

Proceed in the reverse order to removal .