B2CK09K1 - 206 BE4R GEARBOX

CLEANING AND REFITTING CONDITIONS GEARBOX

Do not use abrasives or sharp tools on the joint faces .

Clean the threads and taps .

Fit only parts which are clean and free from faults (scores, burrs, knocks...) .

Oil the parts one by one as they are refitted .

Always renew after removal :

- the seals
- the pins
- the bearings
- the shaft line tightening nuts
- the differential crown wheel tightening bolts
- the 5th speed gear thrust collar
- the input shaft nut lock washer

Maintain the matching of :

- the clutch, gearbox and differential housings
- the selection lever and shaft
- the engagement finger and lever
- the forks and shafts

Preliminary operations :

- operations which must be carried out before beginning the method

Complementary operation(s) :

- operations which must be carried out after completing the method in order to make the gearbox operational again