C5DG0EF1 - 206

REMOVAL - REFITTING RAIN SENSOR

1 - REMOVAL

Remove the mirror (1) by pushing it upwards .

Disconnect the electrical supply (2) .

On each side pull the green calipers (3) to release the rain sensor from the bases on the windscreen .

Do not use sharp tools .

Remove the rain sensor (4) .

IMPERATIVE : do not touch the rain sensor lens or the window on the glass, cleanness is essential for correct operation ( the sensor and the glass must be clean) .

2 - REFITTING

During replacement, do not touch the rain sensor lens once the protective cover is removed, or the window in the screen printing (A) once the plastic film is removed .

Maintain pressure to compress the seal .

Simultaneously lock the the two green calipers (3) on the bases .

Proceed in the reverse order to removal .

Check operation by spraying water on the detection zone with the wiper stalk in the AUTO position (e.g. variable speed wipe) .

WARNING : do not clean the screen when the AUTO function is selected .