B1FB01K1 - 206 TU ENGINE DW10TD ENGINE D4D ENGINE MERCOSUR

DATA - TIGHTENING TORQUES - LUBRICATION

1 - OIL CAPACITY

IMPERATIVE : engine ; always check the oil level using the dipstick .

EW/DW ENGINE D4D ENGINE

engine | EW10J4 | DW8 - DW8B | DW10TD | D4D
--- | --- | --- | --- | ---
special features | without | without | without | without
oil capacity with replacement of the oil filter | 4.25 litre(s) | 4.75 litre(s) | 4.5 litre(s) | 3.75 litre(s)
oil capacity without replacement of the oil filter | 4.0 litre(s) | - | - | -
capacity between min and max on the dipstick | - | 1.5 | - | -
always check the oil level using the dipstick

Average oil consumption per 1000 km (600 miles) when the engine is run in : 0.5 litre(s) .

2 - OIL PRESSURE

EW/DW ENGINE

engine | EW10J4 | DW8 - DW8B | DW10TD
--- | --- | --- | ---
check 1 at 1000 rpm minimum pressure (bars) | 1.5 | 1.8 | 2
check 2 at 2000 rpm minimum pressure (bars) | - | 3.7 | 2.8
check 3 at 3000 rpm minimum pressure (bars) | 5 | 4.3 | 3.7
check 4 at 4000 rpm minimum pressure (bars) | - | 4.5 | 4
the values given are in bars for an engine which is run in, at an oil temperature of 80 ° C

D4D ENGINE

engine | D4D
--- | ---
check 1 at 1000 rpm minimum pressure (bars) | 1.55
check 2 at 2000 rpm minimum pressure (bars) | 4
check 4 at 4000 rpm minimum pressure (bars) | 4.35

3 - TIGHTENING TORQUE(S)

TU ENGINE

Aluminium cylinder block .

Cast-iron cylinder block .

engine | TU | TU
--- | --- | ---
special features | aluminium cylinder block | cast-iron cylinder block
(10) pre-tightening, oil pump (da.Nm) | - | -
(10) oil pump (da.Nm) | 0.9 | -
(11) pre-tightening, sump (da.Nm) | - | -
(11) sump (da.Nm) | 0.8 | -
(12) oil pressure switch (da.Nm) | 2.5 | -
(13) filter nipple (da.Nm) | 0.8 | -
(14) drain plug (da.Nm) | - | -

EW/DW ENGINE

EW10J4 engine .

DW8 / DW8B engine .

engine | EW10J4 | EW10J4 | DW8 - DW8B
--- | --- | --- | ---
special features | temperate climates | hot countries | without
(10) pre-tightening, oil pump (da.Nm) | - | - | -
(10) oil pump (da.Nm) | 0.9 | 0.9 | 1.6
(11) pre-tightening, sump (da.Nm) | - | - | -
(11) sump (da.Nm) | 0.8 | 0.8 | 1.6
(12) oil pressure switch (da.Nm) | 3 | 3 | 3
(13) filter nipple (da.Nm) | 0.8 | 5.0 | 5.0
(14) drain plug (da.Nm) | 3.4 | 3.4 | 3.4

DW10TD ENGINE

DW10TD engine .

engine | DW10TD
--- | ---
special features | without
(10) pre-tightening : oil pump (da.Nm) | -
(10) oil pump (da.Nm) | 1.6
(11) pre-tightening : sump (da.Nm) | -
(11) sump (da.Nm) | 1.6
(12) oil pressure switch (da.Nm) | 3.0
(13) filter nipple (da.Nm) | 5.0
(14) drain plug (da.Nm) | 3.4
(15)housing output lubrication pipe | 2.2
(16)turbo inlet lubrication pipe | 4.7
(17)turbo outlet lubrication pipe | 1.2
(18)housing inlet lubrication pipe | -

D4D ENGINE

engine | DW10TD - TU3JP - TU5JP4 - EW10J4 - D4D
--- | ---
special features | without
oil pressure switch (da.Nm) | 3