B1GG0SK1 - 206 DW8 ENGINE

REMOVAL - REFITTING RADIATOR AND FAN ASSEMBLY MOUNTING

1 - REMOVAL

Remove the fastener (1) for the earth lead .

drain the cooling system .

Remove :

- the radiator grille
- the fasteners (3)
- the coolant hoses
- the cooling radiator (from above)
- the air filter and its connections
- the bolts (4)

Unfasten the grille .

WARNING : do not scratch the paintwork or bend the wing .

AIR CONDITIONING

Remove the bolts (6) (Dehydrator reservoir) .

IMPERATIVE : move aside the condenser and dryer tank assembly without opening the refrigerant circuit .

ALL MODELS

According to specification :

- rotate the union (7) a quarter turn upwards
- remove the hose (7)

Remove :

- the maxi-fuse
- the plate (8)
- the connector (9) (upwards)

Disconnect the connector (10) .

Remove :

- bonnet lock (11)
- the bolts (12)
- radiator and fan assembly mounting (from above)

2 - REFITTING

Proceed in the reverse order to removal .

fill and bleed the cooling system .