B1GG0XK1 - 206

REMOVAL - REFITTING COOLANT PUMP

1 - REMOVAL

DRAIN THE COOLING SYSTEM .

REMOVE THE TIMING BELT .

Remove the 4 bolts (1) .

IMPERATIVE : do not slacken the securing bolts (2) .

Remove the coolant pump .

2 - REFITTING

IMPERATIVE : check that the centralising dowels are present on the cylinder block .

Refit the coolant pump after first coating the pipe seal (3) with grease .

Replace the 4 bolts (1) .

Tightening torque(s) :

- pre-tightening : 0.4 da.Nm
- tightening : 1.4 da.Nm

REFIT THE TIMING BELT .

FILL AND BLEED THE COOLING SYSTEM .