C5ID0BF1 - 206 CABRIOLET

CHECK HYDRAULIC PUMP OIL LEVEL

remove the upper trim from the control unit .

Detach the retaining straps (1) .

Remove the cowling (2) .

Place the hydraulic pump (3) in the vertical position .

The oil level on the mark (4) must be between the minimum (B) and maximum mark (A) .

If the oil level is too low, top up via the screw (5) .

IMPERATIVE : use ARAL VITAMOL ZMH type oil .

WARNING : never modify the clip (6) .

Tighten the filler screw (5) : 0.9 ± 0.1 da.Nm .

Test operation .

Check the oil level again .

If the oil level is above the maximum mark (A), drain the oil using the drain screw (7) .

Proceed in the reverse order to removal .

Fit : the ecu upper trim .