C5HG1GK1 - 206

REMOVAL - REFITTING HEATER PANEL

1 - REMOVAL

Remove :

- the upper central panel (1)
- the centre panel (2)
- the radio (according to specification)

Remove the fasteners (3) .

Press on the air conditioning control panel at point (A) to tilt it towards the interior .

Release the control panel (4) from its housing .

Remove the clips (5), (6), (7) to release the cables .

Unclip the connector (8) .

Remove the air conditioning panel .

Standard version .

Unclip : The connectors (9), (10) .

Remove the air conditioning panel (11) .

2 - REFITTING

WARNING : on the single air conditioning version, reconnect the connector (8) before the fixings of the heater control panel .

Proceed in the reverse order to removal .