C5CG0YF1 - 206

REMOVAL - REFITTING SCREEN BLIND SUB-ASSEMBLY

IMPERATIVE : store the concealing blind in its housing .

Remove the headlining .

1 - REMOVAL

Disconnect the electrical connection .

Remove :

- the roof console bracket (1)
- the 16 bolts (2) around the edge of the sub-assembly (3)

NOTE : two people are required to perform the following operation .

Unclip the sub-assembly (3) at the front (areas A and B) and remove it through the rear of the vehicle .

2 - REFITTING

Position the sub-assembly (3) by means of the front and rear pins (4) and (5) .

Continue the fitting operations in the reverse order to removal .