C4CG25F1 - 206 CABRIOLET

REMOVAL - REFITTING : REAR QUARTER PANEL EXTERIOR WEATHERSTRIP

1 - REMOVAL

Place the vehicle in cabriolet position .

IMMOBILISE THE BOOT COVER .

Remove the clip (1) .

Lift the rear section of the weatherstrip (2) (A) .

Detach the weatherstrip (2) forwards (B) .

Detach the weatherstrip (2) .

2 - REFITTING

NOTE : apply a product to assist fitting on the flange (example: soapy water) .

Engage the weatherstrip (2) on the flange (C) .

Gradually fit the seal as far as the other end .

Fit a new clip (1) .

Continue the fitting operations in the reverse order to removal .