C5EG0BF1 - 206

REMOVAL - REFITTING HEADLAMPS

1 - REMOVAL

Remove :

- the grille
- the fasteners (1)
- the electrical connections
- the headlamp

2 - REFITTING

Position the headlight aligning plate (2) on the shaft (3) .

Make the electrical connections .

Engage the headlight until the guide (4) penetrates the flanged edge of the wing .

Tighten the bolts in the following order : A, B, C .

Fit the grille .

Check :

- the electrical operation
- the adjustment of the lamps