B3CB0IK1 - 206

IDENTIFICATION, DATA, TIGHTENING TORQUE(S) FRONT SUSPENSION

1 - IDENTIFICATION

(1) {{N12559}} fixation de tige d'amortisseur .

(2) Engine sub-frame front fastener .

(3) {{N12560}} fixation avant de bras inférieur .

(4) {{N12561}} fixation de transmission .

(5) {{N12562}} fixation rotule de biellette de connexion .

(6) {{N12563}} fixation arrière de bras inférieur .

(7) Anti-roll bar .

(8) Engine sub-frame rear fastener .

(9) {{N12564}} réglage de biellette de connexion .

(10) {{O32866}} fixation rotule inférieure de pivot .

(11) {{N12565}} fixation corps d'amortisseur sur pivot .

2 - DATA

2 - 1 - FRONT ANTI -ROLL BAR

engine code | HFX - HFZ KFW - WJZ - WJY | HFX - HFZ WJZ - WJY | HFX - HFZ - KFW WJZ - WJY - 7LZ
--- | --- | --- | ---
special features | without | 'Affaire' | overseas export
anti-roll bar diameter (mm) | 18 | 18 | 18

engine code | NFZ - NFU - RHY | NFZ - NFU - RHY
--- | --- | ---
special features | without | overseas export
anti-roll bar diameter (mm) | 19 | 19

engine code | KFX | RFR | RFR - NFU
--- | --- | --- | ---
special features | LPG | without | coupe-cabriolet
anti-roll bar diameter (mm) | 18 | 20 | 20

Attention : phrase vide (a renseigner) .

2 - 2 - FRONT AXLE ANGLES

engine code | HFX - HFZ | HFX - HFZ - KFW | HFX - HFZ
--- | --- | --- | ---
special features | conventional steering 165/70 R13 | power steering 165/70 R13 | conventional steering 175/65 R14
H1 (mm) +12 / -8 | 122 | 122 | 123
track / wheel (mm) ± 0.5 | -0.75 | -0.75 | -0.75
track / wheel (°) ± 5' | -0° 7' | -0° 7' | -0° 7'
camber ± 30' | 0° | 0° | 0°
castor ± 30' | 2° 16' | 3° 16' | 2° 16'
pivot angle ± 30' | 9° 31' | 9° 31' | 9° 42'

engine code | HFX - HFZ - 8HX KFW - NFZ WJZ - WJY - RHY | RHY - NFU
--- | --- | ---
special features | power steering 175/65 R14 | power steering 185/65 R14
H1 (mm) +12 / -8 | 123 | 128
track / wheel (mm) ± 0.5 | -0.75 | -0.75
track / wheel (°) ± 5' | -0° 7' | -0° 7'
camber ± 30' | 0° | 0°
castor ± 30' | 3° 16' | 3° 16'
pivot angle ± 30' | 9° 42' | 9° 42'

engine code | RFR | RFR
--- | --- | ---
special features | power steering 185/55 R14 | power steering 195/45 R16
H1 (mm) +12 / -8 | 120 | 129
track / wheel (mm) ± 0.5 | -0.75 | -0.75
track / wheel (°) ± 5' | -0° 7' | -0° 7'
camber ± 30' | 0° | 0°
castor ± 30' | 3° 16' | 3° 16'
pivot angle ± 30' | 9° 42' | 9° 42'

engine code | KFX | NFU - RFN
--- | --- | ---
special features | LPG 175/65 R14 | coupe/cabriolet 185/55 R15
H1 (mm) +12 / -8 | 133 | 120
track / wheel (mm) ± 0.5 | -0.75 | -0.75
track / wheel (°) ± 5' | -0° 7' | -0° 7'
camber ± 30' | 0° | 0°
castor ± 30' | 3° 24' | 3° 13'
pivot angle ± 30' | 9° 31' | 9° 42'

'Affaire'
engine code | HFX - HFZ | HFX - HFZ
--- | --- | ---
special features | power steering 165/70 R13 | conventional steering 165/70 R13
H1 (mm) +12 / -8 | 122 | 122
track / wheel (mm) ± 0.5 | -0.75 | -0.75
track / wheel (°) ± 5' | -0° 7' | -0° 7'
camber ± 30' | 0° | 0°
castor ± 30' | 3° 44' | 2° 44'
pivot angle ± 30' | 9° 31' | 9° 31'

'Affaire'
engine code | WJZ - WJY | WJZ - WJY
--- | --- | ---
special features | power steering 175/65 R14 | conventional steering 175/65 R14
H1 (mm) +12 / -8 | 123 | 123
track / wheel (mm) ± 0.5 | -0.75 | -0.75
track / wheel (°) ± 5' | -0° 7' | -0° 7'
camber ± 30' | 0° | 0°
castor ± 30' | 3° 33' | 2° 33'
pivot angle ± 30' | 9° 42' | 9° 42'

overseas export
engine code | HFX - HFZ - KFX K6C - NFZ - NFU - WJZ WJY - RHY - 7LZ | HFX - HFZ - KFX - K6C WJZ - WJY - 7LZ
--- | --- | ---
special features | power steering 175/65 R14 | conventional steering 175/65 R14
H1 (mm) +12 / -8 | 148 | 148
track / wheel (mm) ± 0.5 | -0.75 | -0.75
track / wheel (°) ± 5' | -0° 7' | -0° 7'
camber ± 30' | 0° 7' | 0° 7'
castor ± 30' | 3° 05' | 2° 07'
pivot angle ± 30' | 9° 20' | 9° 20'

NOTE : these values are for a reference height (H1) .

3 - {{N12566}} VALEURS DE PARALLELISME AVEC UN VEHICULE EN ORDRE DE MARCHE

3 - 1 - {{N12519}} VEHICULES EQUIPES DE PNEUMATIQUES 165/70 R13

(H) Height between the ground and the jacking point (In mm) .

(H1) Height from ground to front jacking bracket at reference height .

(P) Tracking at the axle (Tolerance ± 1 mm) .

3 - 2 - {{N12519}} VEHICULES EQUIPES DE PNEUMATIQUES 175/65 R14 - 185/55 R15 - 195/45 R16 ({{N12567}} SAUF VEHICULES GRAND EXPORT)

(H) Height between the ground and the jacking point (In mm) .

(H1) Height from ground to front jacking bracket at reference height .

(P) Tracking at the axle (Tolerance ± 1 mm) .

3 - 3 - {{N12568}} TOUS TYPES VEHICULES GRAND EXPORT

(H) Height between the ground and the jacking point (In mm) .

(H1) Height from ground to front jacking bracket at reference height .

(P) Tracking at the axle (Tolerance ± 1 mm) .

4 - TIGHTENING TORQUES

(2) Engine sub-frame front fastener : 11 da.Nm .

(3) {{N12560}} fixation avant de bras inférieur : 11 da.Nm .

(6) {{N12563}} fixation arrière de bras inférieur : 11 da.Nm .

(8) Engine sub-frame rear fastener : 11 da.Nm .

(10) Pivot ball joint : 4 da.Nm .

(11) Pivot clamp mounting : 5.5 da.Nm .

(12) Anti-roll bar link fixing : 3.5 da.Nm .

(13) Anti-roll bar link fixing : 3.5 da.Nm .

(14) Anti-roll bar bearing fixing : 10.5 da.Nm .

(15) Shock absorber mounting to body fastener : 2.5 da.Nm .