B2CG59K1 - 206 MA GEARBOX

ASSEMBLY GEARBOX

1 - SPECIAL TOOLS

reference | description | reference | reference
--- | --- | --- | ---
[1] | fitting drift for final drive right-hand output oil seal | (-).0317-U | 7114-T.X
[2] | fitting drift for final drive left-hand output oil seal | (-).0317-T | 7114-T.W

2 - ASSEMBLY

Place the gearbox on a block of wood (H = 180 mm) .

Fit :

- the speedometer pinion (1)
- the reverse lamp switch (2)

1st fitting, Fit :

- the connecting plate (3)
- the clamp (4)
- the ball joint lever (5), with the ball joint greased

2nd fitting :

- refit the selection relay lever (6)

Lightly coat with MOLYKOTE BR2 PLUS (G10) grease :

- the splines (A) of the input shaft of gearboxes manufactured up to 02/01/95
- the clutch release bearing guide (B)

WARNING : an excess of grease on the splines of the input shaft may damage the clutch .

Refit the clutch stop (7) .

Fill the space between the oil seal lips with grease .

Fit :

- the final drive right hand output lip seal using the tool [1]
- the final drive left hand output lip seal ; using the tool [2]