B1DB3FK1 - 206 DW10TD ENGINE

IDENTIFICATION - DATA CYLINDER HEAD GASKET

1 - IDENTIFICATION

1 - 1 - 1ST FITTING : CYLINDER HEAD GASKET ELRING

(A) : Thickness identification .

1 - 2 - 2ND FITTING : CYLINDER HEAD GASKET REINZ

(B) : thickness identification .

2 - DATA

There are 5 categories of laminated metal cylinder gaskets .

piston protrusion measurements (mm) | thickness (mm) | notch(es) : at (A) or (B)
--- | --- | ---
0.47 to 0.605 | 1.30 ± 0.06 | 1
0.605 to 0.655 | 1.35 ± 0.06 | 2
0.655 to 0.705 | 1.40 ± 0.06 | 3
0.705 to 0.755 | 1.45 ± 0.06 | 4
0.755 to 0.83 | 1.50 ± 0.06 | 5

IMPERATIVE : if the value measured does not correspond to the values indicated, investigate the origin of the fault (measurement error, handling error etc.) .