B1HJ04K1 - 206 DW10TD ENGINE

CLEANING UNIONS ON THE HIGH PRESSURE FUEL DIRECT INJECTION RAIL

IMPERATIVE : when carrying out an operation on the diesel circuit, respect safety instructions .

1 - PRELIMINARY OPERATIONS

Disconnect the battery .

Remove the style cover .

Protect the alternator .

2 - METHOD OF OPERATION

Cleaning of the repair areas (At (A)) :

- dip the brush in the product SODIMAC n°35
- clean the points (A) using the product and draw up simultaneously using suction equipment
- clean the vacuum extractor after use