C5HG1EK1 - 206 TU ENGINE

REMOVAL - REFITTING AIR CONDITIONING COMPRESSOR

1 - REMOVAL

Drain the refrigerant circuit .

Remove the ancillary drive belt .

Remove the bolt (1) .

Disconnect the compressor inlet and outlet pipes .

IMPERATIVE : quickly seal the compressor inlets and outlets and the pipes .

Disconnect the connector (2) .

Remove the securing bolts (3) .

Remove the compressor .

2 - REFITTING

TU1JP ENGINE TU3JP ENGINE

Check that the pins (4) are present .

TU5JP ENGINE

Check that the pins (4) are present .

ALL MODELS

Gently push back the pins (4) into their housing .

Refit the compressor .

IMPERATIVE : tighten the securing bolts to the required torque value starting with the front bolts (3) .

Tightening torque : 2.5 da.Nm .

Re-connect the connector (2) .

IMPERATIVE : reconnect all the connectors fitted with new seals, lubricated with compressor oil .

Tighten the bolt (1) to 4 da.Nm .

Fit the ancillary drive belt .

Charge the refrigerant circuit .