B--B00F1 - 206

RECOMMENDED PRODUCTS MECHANICAL

1 - CLEANING PRODUCTS

applications - data | suffix : | products Part No. | supplier(s)
--- | --- | --- | ---
gelatinous liquid to be used for stripping joint faces and non-metallic joints | D2 | DECAPLOC 9731.25 | FRAMET
aerosol spray to be used for unsticking and stripping joint faces and non-metallic joints | DECAPJOINT 9732.11
degreaser SD 140 | D3 | 9736.57 | -

2 - SEALING COMPOUNDS

applications - data | suffix : | products Part No. | supplier(s)
--- | --- | --- | ---
locking and sealing threaded assemblies which must remain removable | E3 | FRENETANCH 9732.48 | FRAMET
sealing unions and joint faces | E4 | FORMETANCH 9732.46
securing bearings, snap rings, sockets, sleeves, inserts, pulleys strengthening fluted and feathered engagements | E5 | SCELBLOC 9732.47
locking and sealing of studs, bolts, nuts, with maximum efficiency | E6 | FRENBLOC 9733.10
sealing of joint faces, replacing traditional seals | E7 | FORMATJOINT 9732.45
sealing of porous points on the cylinder block : aluminium based | E8 | POXY MATIC 9732.17
sealing of joint faces subjected to high pressures and vibrations remains flexible after drying | E10 | AUTOJOINT OR 9735.66
sealing of exhaust connections (except ball joints) | E11 | ECHAPNET 9735.01
strengthening of fixed assemblies : sealing | E12 | AUTO FORM 549 9733.68
flexible joint capable of withstanding atmospheric agents | E13 | AUTO JOINT CLAIR 9731.61
tight locking of threads bonding of caps to the cylinder block and cylinder head | E14 | LOCTITE 275 9735.58
sealing of joint faces, replacing traditional seals | E15 | FORMATJOINT 9732.45

3 - RELEASING AGENTS

applications - data | suffix : | products Part No. | supplier(s)
--- | --- | --- | ---
rusted or corroded parts and assemblies which have seized (in aerosol form) | F1 | 9731.68 | SADAPS - BARDHAL

4 - LUBRICANTS

applications - data | suffix : | products Part No. | supplier(s)
--- | --- | --- | ---
grease with high adhesive capacity : grease for use mainly on the drive shafts | G1 | MOBIL 525 9732.03 | CEPAC
grease with high adhesive capacity : grease which can be used on mechanisms subjected to high pressures and water splashes | MECAGRAISSE 9733.69
heat resistant grease : grease to be used on the ball joints of the exhaust manifolds | G2 | LUBRITHERM G200 9733.44
lubricant for arduous conditions : lubricant to be used on mechanisms subjected to water splashes, high pressures and extreme temperatures | G3 | LUBRITHERM G200 9733.44
heat resistant grease : lubricant to be used on threaded parts fitted to the cylinder head (spark plugs) | G4 | LUBRITHERM G200 9733.44
multi-purpose grease : grease to be used for routine work | G6 | 9735.72 | CEPAC
special purpose grease : grease to be used on anti-roll bar bearings | G7 | ESSO NORVA 275 9734.14
special purpose grease : grease to be used when fitting ABS sensors | G9 | ESSO NORVA 275 9734.14
Molykote G. Rapid plus grease : grease to be used when fitting cylinder head bolts | G10 | MOLYKOTE G 9732.05
lubricant for sliding the windows in the door seal | G11 | KRYTOX.GPL103 9718.78
grease for surfaces | G12 | MOLYKOTE BR2+ 9731.89
multi-purpose grease (drive shafts RZEPPA) (steering rack) | G13 | TOTAL N3945 9735.D2

5 - HYDRAULIC MINERAL FLUID

applications - data | suffix : | products Part No. | supplier(s)
--- | --- | --- | ---
hydraulic fluid for electric hood motor | M1 | ESSO UNIVIS J32 9735.57 | CEPAC