B2CG82K1 - 206 AL4 AUTOMATIC GEARBOX

REMOVAL - REFITTING AUTOMATIC GEARBOX OIL PRESSURE SENSOR

1 - REMOVAL

NOTE : do not drain the gearbox .

Remove :

- the ECU cover
- the connector of the engine ecu
- the battery
- the battery container
- the air cleaner housing
- the air hose

Remove the 2 bolts (1) (Mounting of the modular connector on the gearbox) .

Disconnect the modular connector (2) .

Extract the green 3-way connector (3) from the modular connector (2) .

Remove :

- the front left-hand wheel
- the front left mud shield
- the oil pressure sensor harness (4)
- the 2 oil pressure sensor (4) fixing bolts
- (4) automatic gearbox oil pressure sensor

2 - REFITTING

Replace the sensor o ring (4) .

Fit :

- (4) automatic gearbox oil pressure sensor
- the 2 oil pressure sensor (4) fixing bolts : tightening torque 1 da.Nm
- the oil pressure sensor harness (4)
- the green 3-way connector (3) in the modular connector (2)
- the 2 bolts (1) : tightening torque 1 da.Nm

Reconnect the modular connector (2) .

Fit :

- the battery container
- the battery
- the air cleaner housing
- the air hose
- the front left mud shield
- the front left-hand wheel
- the connector of the engine ecu
- the ECU cover

Connect the battery .