C4DG0KF1 - 206 CABRIOLET

REMOVAL - REFITTING FRONT MOVING PANEL

1 - REMOVAL

Change the vehicle into the coupé version .

Lower the side windows of the doors and rear quarter panels .

THE INJECTION PUMP HOUSING .

IMMOBILISE THE BOOT COVER .

Lift the roof then place it in the intermediate position for accessibility (Two operators are necessary) .

{{N5660}} DEPOSER LES GARNITURES LATERALES DE PAVILLON .

{{N12379}} repérer de chaque côté la position de l'équerre (At (A)) .

NOTE : {{n12380}} effectuer la reconstruction du toit lors du remplacement du panneau mobile avant .

Remove the fixings (1) from the support .

Remove the front moving panel (Two operators are necessary) .

2 - REFITTING

Proceed in the reverse order to removal .

Tighten the fasteners (1) to 0.95 ± 0.15 da.Nm .

Test operation .

CHECK THE SEALING OF THE ROOF .