C4CG1YF1 - 206 CABRIOLET

REMOVAL - REFITTING BOOT STRUT

1 - REMOVAL

Remove :

- THE REAR SEAT
- THE REAR SEAT BACK REST
- THE REAR QUARTER PANEL SIDE TOP TRIM
- THE REAR QUARTER PANEL SIDE TRIM PANEL
- the rear seat belt housing

Open the luggage compartment .

Uncouple the strut (1) at the top leaving the clip on the strut body .

Uncouple the strut (1) at the bottom .

Detach then remove the strut .

2 - REFITTING

Proceed in the reverse order to removal .

Tighten the rear seat belt housing bolt to 3 ± 1 dan.m .

Test operation .