B3DJ09K1 - 206

OVERHAUL REAR HUBS (DRUM)

1 - SPECIAL TOOLS

[1] Drift for removing and fitting hub bearing (-).0539 T .

2 - REMOVAL

REMOVE THE REAR HUB .

Remove the bearing retaining circlip (1a) or ring (1b) .

Press out the bearing using the tool [1] .

3 - REFITTING

Clean the hub .

Use genuine new parts, coat them with grease .

Coat the outside of the bearing with grease to make fitting easier .

Press the bearing fully home using the tool [1] .

Refit the bearing retaining circlip or ring .

REFIT THE DRUM/HUB .