C4BH2YF1 - 206 CABRIOLET

REPLACEMENT OF THE REAR WHEEL ARCH ASSEMBLY

IMPERATIVE : this vehicle has been designed using the mig brazing process technique ; when the structure is repaired, all the connections concerned must be welded using the same procedure ; any other technique is prohibited .

WARNING : all the scoured areas must be protected by the approved electrolytic re-zincing process .

IMPERATIVE : observe elementary health and safety rules (wearing of filter mask for organic fumes - work in a ventilated area) .

1 - COMPLEMENTARY OPERATION(S)

Replacement :

- REAR WING

2 - IDENTIFICATION OF REPLACEMENT PARTS

Rear wheel arch assembly .

3 - COMPOSITION

(1) : Rear wheel arch .

(2) : Rear wheel arch (Rear section) .

(3) : Rear bumper bracket .

4 - PART(S) REQUIRED TO CARRY OUT THE OPERATION

Rear wheel arch assembly .

5 - PREPARATION OF THE NEW PART

6 - CUTTING OUT

7 - RELEASING

8 - WELDING

9 - SEALING

10 - PROTECTION