B1DF02K1 - 206 D4D ENGINE MERCOSUR

ROCKER ADJUSTMENT

1 - REMOVAL

Remove the battery tray .

Disconnect the battery .

Remove :

- the style cover
- the air cleaner

Remove :

- the compact coil unit (1)
- the air distributor (2)
- the cylinder head cover

2 - ROCKER ADJUSTMENT

Method of adjusting the exhaust valve at the outlet .

Adjustment values (Cold) :

- inlet : 0,10 mm
- exhaust : 0,20 mm

exhaust valve full opening (A) | intake valve setting (B) | exhaust valve setting (C)
--- | --- | ---
1 | 3 | 4
3 | 4 | 2
4 | 2 | 1
2 | 1 | 3

3 - REFITTING

apply sealant E10 to the bearings 1 - 5 of the camshaft at (D) .

apply sealant E10 to the 4 holes fixing the cylinder head cover at (E) .

Replace the cylinder head bolts and offer them up manually .

Tighten the bolts to 1 da.Nm. in the order indicated .

Refit new plug recess seals using a 30 mm socket .

Fit :

- the air distributor
- the compact coil unit

Proceed in the reverse order to removal .