C4CG21F1 - 206 CABRIOLET

REMOVAL-REFITTING OF THE EXTERIOR MIRROR

1 - REMOVAL

REMOVE THE INTERIOR CHEATER (1) .

Disconnect the tweeter (A) .

Disconnect the connector (2) .

Remove the fasteners (3) (4) .

Unclip the exterior mirror and remove it .

2 - REFITTING

Clip the mirror .

Proceed in the reverse order to removal .

WARNING : when tightening the mirror fasteners, ensure that the exterior cheater of the mirror is placed on its seal .

Test operation .