C5JG09F1 - 206

REMOVAL - REFITTING REAR SEAT BELTS

1 - REMOVAL

Remove :

- the fastener (1)
- the trim (2)
- the rivet (3)

Detach the trim (4) .

Remove :

- the fasteners (5) - (6)
- the quarter light surround

Remove the fastener (7) .

2 - REFITTING

Proceed in the reverse order to removal .

3 - TIGHTENING TORQUES

Tighten the fastener (1) to 3 daN.m. .

Tighten the fastener (6) to 3 daN.m. .

Tighten the fastener (7) to 3 daN.m. .