B1FB0IK1 - 206

RECOMMENDATIONS LUBRICANTS

1 - OIL QUALITIES

The engine lubrication oils are categorised in accordance with 3 quality levels :

- mineral oil(s) (ESSO UNIFLO, TOTAL ACTIVA/QUARTZ 5000)
- semi-synthetic oil(s) (ESSO ULTRA, TOTAL ACTIVA/QUARTZ 7000)
- synthetic oil(s) (ESSO ULTRON, TOTAL ACTIVA/QUARTZ 9000)

In addition to the existing range of oils, for vehicles from model year 2000, an "energy saving" oil is available; This oil contributes to the objective of resolving the problem of fuel consumption, which is Peugeot's aim .

IMPERATIVE : the energy saving oil must not be used in engines prior to 2000 Model Year, nor in engines XU10J4RS, DW12TED4, EW12J4, 1580 SPI or SOFIM engines ; likewise, 0W30 oil must not be used in the above mentioned engines .

Automobiles PEUGEOT recommends the quality of lubricants to use in the owner's documentation :

- handbook
- warranty and maintenance record

WARNING : for vehicles sold from model year 1999, in accordance with the normal maintenance plan, the use of an approved semi-synthetic oil is imperative .

Organisations categorise the oils in accordance with their performance and give them a quality label which is visible on the packaging :

- API : American Petroleum Institute
- ACEA : European Automobile Manufacturers' Association
- NLGI : National Lubrication Grease Institute

The grade (viscosity index) must be selected in accordance with the climate of the country of use .

2 - RECOMMENDED LUBRICANTS AND PERFORMANCE SPECIFICATIONS FOR INDIVIDUAL UNITS

2 - 1 - PUMPS

units | ESSO | API standards | ACEA standards
--- | --- | --- | ---
KF - KF1 - KF2 - KF6 - KF5 - XN2 petrol injection pump | ESSOLUBE X101 10W Part No. 9730.GA (1) | SC/CC | -
vacuum pump (with separate lubrication) PIERBURG | ESSO UNIFLO 10W40 | SJ | A2
vacuum pump (with separate lubrication) SAGINAW | ESSO GEAR OIL GX 80W90 | GL5 | -
power steering pump | ESSO ATF D (1) Part No. 9730.94 | - | -
(1) marketed by Parts Department in 2 litre cans

units | TOTAL | API standards | CCMC/ standards ACEA
--- | --- | --- | ---
KF - KF1 - KF2 - KF5 - KF6 - XN2 petrol injection pump | TOTAL RUBIA S 10W TOTAL RUBIA H 10W | CD/SF CC/SF | D2 D1
vacuum pump (with separate lubrication) PIERBURG | TOTAL ACTIVA 7000 10W40 TOTAL QUARTZ 7000 10W40 | SJ/CF | A3/B3
vacuum pump (with separate lubrication) SAGINAW | TOTAL TRANSMISSION TM MULTIGRADE 80W90 TOTAL TRANSMISSION TM 80W90 | GL5 | -
power steering pump | TOTAL FLUIDE AT42 | - | -

units |  | API standards | ACEA standards
--- | --- | --- | ---
power steering pump | PENTOSIN CHF 11 S Part No. 9979.64 (1) (2) | - | -
(1) marketed by Parts Department in 1 litre cans (2) for cold climates only, this oil cannot be mixed with other oils; it is therefore necessary to completely drain the system and to rinse it before filling with this oil

2 - 2 - GEARBOX FINAL DRIVE - TRANSFER BOX

units | ESSO | API standards | ACEA standards
--- | --- | --- | ---
BC3 | GX 80W90 | SJ | A2
4HP14 - 4HP18 - MB3 automatic gearbox | ESSO ATF D Part No. 9730.94 (1) (3) | - | -
4HP20/AL4 automatic gearbox | ATF 4HP20/AL4 Part No. 9736.22 (1) (3) | - | -
manual gearbox MA-BE-ME-ML-BA7-BA10 | ESSO GEAR OIL BV 75W80 (1) (3) Part No. 9736.41 | specific to Peugeot | -
405 x 4 transfer box | ESSO GEAR OIL BT 80W90 (1) Part No. 9736.19 | GL5 | -
(1) marketed by Parts Department in 2 litre cans (3) never use any other grade of oil

units | TOTAL | API standards | ACEA standards
--- | --- | --- | ---
BC3 | TM 80W90 | SJ/CF | A3/B3
4HP14 - 4HP18 - MB3 automatic gearbox | TOTAL FLUIDE AT42 | - | -
4HP20 - AL4 automatic gearbox | - | - | -
manual gearbox MA-BE-ME-ML-BA7-BA10 | TOTAL TRANSMISSION BV 75W80 (4) new formula | specific to Peugeot | -
405 x 4 transfer box | TOTAL TRANSMISSION X4 80W90 | GL5 | -
(4) if another oil has been used, drain and rinse but Never Mix the oils

2 - 3 - REAR FINAL DRIVE

units | ESSO | API/PEUGEOT standards
--- | --- | ---
conventional rear axle | ESSO GEAR OIL VT (5) | specific to Peugeot
conventional hypoid rear axle with limited slip and 405 x 4 | ESSO GEAR OIL BT 80W90 (1) Part No. 9736.19 | GL5
(1) marketed by Parts Department in 2 litre cans (5) if there is no ESSO GEAR OIL VT oil available, use ESSO GEAR OIL GP90 or GX-80W90 after emptying and rinsing the final drive, but never mix the two oils

units | TOTAL | API/PEUGEOT standards
--- | --- | ---
conventional rear axle | TOTAL TRANSMISSION TM MULTIGRADE 80W90 (4) TOTAL TRANSMISSION TM 80W90 | GL5
conventional hypoid rear axle with limited slip and 405 x 4 | TOTAL TRANSMISSION X4 80W90 | GL5
(4) if another oil has been used, drain and rinse but Never Mix the oils

2 - 4 - SUSPENSION

units | ESSO | API/PEUGEOT standards
--- | --- | ---
hydraulic suspension | ESSO LHM EXTRA | specific to Peugeot

units | TOTAL | API/PEUGEOT standards
--- | --- | ---
hydraulic suspension | TOTAL LHM PLUS | specific to Peugeot

2 - 5 - REAR SUSPENSION

units | ESSO | API standards
--- | --- | ---
rear suspension J7 - J9 | ESSO GEAR OIL BT 80W90 (1) Part No. 9736.19 ESSO GEAR OIL GX 80W90 | GL5
(1) marketed by Parts Department in 2 litre cans

units | TOTAL | API standards
--- | --- | ---
rear suspension J7 - J9 | TOTAL TRANSMISSION TM MULTIGRADE 80W90 TOTAL TRANSMISSION TM 80W90 | GL5

2 - 6 - STEERING

units | ESSO | API standards
--- | --- | ---
J7 - J9 steering systems except J9 power steering | ESSO GEAR OIL BT 80W90 (1) Part No. 9736.19 ESSO GEAR OIL GX 80W90 | GL5
(1) marketed by Parts Department in 2 litre cans

units | TOTAL | API standards
--- | --- | ---
J7 - J9 steering systems except J9 power steering | TOTAL TRANSMISSION TM MULTIGRADE 80W90 TOTAL TRANSMISSION TM 80W90 | GL5

2 - 7 - SHOCK ABSORBERS

units | ESSO | API standards
--- | --- | ---
front shock absorbers | ESSO OLEOFLUID PA (1) Part No. 9730.27 | specific to Peugeot
(1) marketed by Parts Department in 2 litre cans

2 - 8 - MECHANICAL UNITS

units | ESSO | NLGI standards
--- | --- | ---
mechanical units | ESSO MULTIPURPOSE GREASE 4746 | NLGI2

units | TOTAL | NLGI standards
--- | --- | ---
mechanical units | TOTAL MULTIS 2 | NLGI2

2 - 9 - AIR CONDITIONING COMPRESSORS

units | products | packaging | Part No.
--- | --- | --- | ---
compressors for R12 refrigerant | LUNARIA-S (*) | 125 ml | 9735.H8
compressors SANDEN with fixed displacement for R134a refrigerant | SANDEN SP20 | 40 ml 250 ml | 9735.C8 9735.C6
compressors SANDEN with variable displacement for R134a refrigerant | SANDEN SP10 | 40 ml 250 ml | 9735.C5 9735.C4
compressors DELPHI-HARRISON for V5 refrigerant | UCON 488 | 40 ml 250 ml | 9979.41 9979.40
(*) do not use LUNARIA-S in compressors made by SANDEN or DELPHI

NOTE : for vehicles manufactured and sold in countries where ESSO and TOTAL products are not available, use PEUGEOT locally recommended lubricants .

3 - OILS FOR PETROL ENGINES

3 - 1 - EUROPE

Country | ESSO | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Germany Austria Belgium Spain FRANCE Great Britain Greece Hungary Italy Ireland Luxemburg Netherlands Poland Portugal Czech Republic Slovakia Switzerland Rumania Russia | ESSO UNIFLO ESSO ULTRA ESSO ULTRON ESSO ULTRON (6) ESSO ULTRA (6) | 15W40 10W40 5W40 0W30 5W30 | SJ SJ/SH EC-I SJ/SH EC-I SJ/SH EC-II - | A2 A3 A3 A3 specific to Peugeot
Denmark Finland Norway Sweden | ESSO UNIFLO ESSO ULTRA ESSO ULTRON ESSO ULTRON (6) ESSO ULTRA (6) | 10W40 10W40 5W40 0W30 5W30 | SJ SJ/SH EC-I SJ/SH EC-I SJ/SH EC-II - | A2 A3 A3 A3 specific to Peugeot
(6) this energy saving oil can only be used with engines designed to receive it (from my 2000)

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
FRANCE | TOTAL ACTIVA 5000 TOTAL ACTIVA 7000 TOTAL ACTIVA 9000 TOTAL ACTIVA 9000 (6) | 15W40 10W40 5W40 0W40 5W30 | SJ SJ SJ SJ EC | A2 A3 A3 specific to Peugeot
Germany Austria Belgium Belorussia Bosnia Croatia Denmark Estonia Finland Great Britain Hungary Ireland Italy Latvia Lithuania Luxemburg Macedonia Norway Netherlands Poland Czech Republic Russia Slovenia Sweden Switzerland | TOTAL QUARTZ 5000 TOTAL QUARTZ 7000 TOTAL QUARTZ 9000 TOTAL QUARTZ 9000 TOTAL QUARTZ 9000 (6) | 15W40 10W40 5W40 0W40 5W30 | SJ SJ SJ SJ SJ EC | A2 A3 A3 A3 specific to Peugeot
Bulgaria Cyprus Spain Greece Malta Portugal Rumania | TOTAL QUARTZ 5000 TOTAL QUARTZ 7000 TOTAL QUARTZ 7000 TOTAL QUARTZ 9000 TOTAL QUARTZ 9000 TOTAL QUARTZ 9000 (6) | 15W40 15W50 10W40 5W40 0W40 5W30 | SJ SJ SJ SJ SJ SJ EC | A2 A3 A3 A3 A3 specific to Peugeot
(6) this energy saving oil can only be used with engines designed to receive it (from my 2000)

3 - 2 - AFRICA

Country | ESSO | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Tunisia | ESSO SUPER OIL (7) ESSO ULTRA ESSO ULTRON | 20W50 15W50 5W40 | SJ SJ SJ/SH EC-I | A2 A3 A3
(7) mineral oil(s)

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
all countries | TOTAL QUARTZ 5000 TOTAL QUARTZ 7000 TOTAL QUARTZ 9000 | 20W50 15W50 5W40 | SJ SJ SJ | A2 A3 A3

3 - 3 - SOUTHERN EUROPE

Country | TOTAL | grade | API standards | CCMC/ACEA standards
--- | --- | --- | --- | ---
Turkey | TOTAL QUARTZ 5000 TOTAL QUARTZ 7000 TOTAL QUARTZ 9000 TOTAL QUARTZ 9000 | 20W50 15W50 5W40 0W40 | SJ SJ SJ SJ/SH EC-II | A2 A3 A3 A3

3 - 4 - FRENCH OVERSEAS TERRITORIES

Country | ESSO | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
French West Indies Reunion | ESSO UNIFLO ESSO ULTRA ESSO ULTRON | 15W40 10W40 5W40 | SJ SJ/SH EC-I SH/SH EC-I | A2 A3 A3

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Caribbean Pacific Polynesia Reunion | TOTAL ACTIVA 5000 TOTAL ACTIVA 5000 TOTAL ACTIVA 7000 TOTAL ACTIVA 7000 TOTAL ACTIVA 9000 | 20W50 15W40 15W50 10W40 5W40 | SJ SJ SJ SJ SJ | A2 A2 A3 A3 A3

3 - 5 - MIDDLE EAST

Country | ESSO | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Bahrain United Arab Emirates Kuwait Lebanon Oman Qatar Yemen | ESSO RACING OIL (8) | 10W40 | SJ/SH EC-I | A3
(8) semi-synthetic oil(s)

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Bahrain United Arab Emirates Kuwait Lebanon Oman Qatar Yemen | TOTAL QUARTZ 5000 TOTAL QUARTZ 7000 TOTAL QUARTZ 9000 | 20W50 15W50 5W40 | SJ SJ SJ | A2 A3 A3

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Iran | TOTAL QUARTZ 5000 | 20W50 | SJ | A2

3 - 6 - SOUTH-EAST ASIA

Country | ESSO | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Australia China Korea Hong Kong India Indonesia Malaysia Singapore Taiwan Thailand Vietnam | ESSO ULTRAFLO ESSO ULTRON | 10W40 5W40 | SJ/SH EC-I SJ/SH EC-I | A3 A3
Australia Thailand | ESSO SUPERFLO | 20W50 | SJ | A2
JAPAN | ESSO ULTRAFLO ESSO ULTRON UNOIL GX-7 UNOIL GX-6 | 10W40 5W40 5W40 10W40 | SJ/SH EC-I SJ/SH EC-I SI/S4 EC-I SJ/S4 EC-I | A3 A3 A3 A2
Hong Kong | ESSO ULTRON | 0W30 | SJ/SH EC-II | A3

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
China India Indonesia JAPAN Malaysia Singapore Taiwan Thailand Vietnam | TOTAL QUARTZ 5000 TOTAL QUARTZ 5000 TOTAL QUARTZ 7000 TOTAL QUARTZ 7000 TOTAL QUARTZ 9000 | 20W50 15W40 15W50 10W40 5W40 | SJ SJ SJ SJ SJ | A2 A2 A3 A3 A3

3 - 7 - SOUTH AMERICA

Country | ESSO | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Brazil | ESSO ULTRA ESSO ULTRON | 15W50 5W40 | SJ SJ/SH EC-I | A3 A3
Argentina Bolivia Paraguay Uruguay | ESSO UNIFLO ESSO ULTRA ESSO ULTRON | 15W40 10W40 5W40 | SJ SJ/SH EC-I SJ/SH EC-I | A2 A3 A3
Chile Columbia Ecuador Surinam | ESSO ULTRON | 5W40 | SJ/SH EC-I | A3

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Argentina Chile Bolivia Brazil Paraguay Uruguay | TOTAL QUARTZ 5000 TOTAL QUARTZ 5000 TOTAL QUARTZ 7000 TOTAL QUARTZ 7000 TOTAL QUARTZ 9000 | 20W50 15W40 15W50 10W40 5W40 | SJ SJ SJ SJ SJ | A2 A2 A3 A3 A3

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Cuba | TOTAL QUARTZ 5000 TOTAL QUARTZ 7000 TOTAL QUARTZ 9000 | 20W50 15W50 5W40 | SJ SJ SJ | A2 A3 A3

3 - 8 - CENTRAL AMERICA AND THE CARIBBEAN

Country | ESSO | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Bahamas Barbados Belize Guatemala Haiti Honduras Jamaica Mexico Panama Puerto Rico Dominican Republic Salvador Trinidad and Tobago | ESSO ULTRON | 5W40 | SJ/SH EC-I | A3

4 - OILS FOR DIESEL ENGINES

4 - 1 - EUROPE

Country | ESSO | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Germany Austria Belgium Spain FRANCE Great Britain Greece Ireland Italy Luxemburg Netherlands Portugal Russia Switzerland | ESSO UNIFLO DIESEL ESSO ULTRA DIESEL ESSO ULTRON DIESEL ESSO ULTRA (6) | 15W40 10W40 5W40 5W30 | CF CF CF - | B2 B3 B3 specific to Peugeot
Hungary Norway Poland Czech Republic Rumania Slovakia | ESSO UNIFLO DIESEL ESSO ULTRA DIESEL ESSO ULTRA (6) | 15W40 10W40 5W30 | CF CF - | B2 B3 specific to Peugeot
Finland | ESSO ULTRA DIESEL ESSO ULTRA (6) | 10W40 5W30 | CF - | B3 specific to Peugeot
Denmark Sweden | - | - | - | -
(6) this energy saving oil can only be used with engines designed to receive it (from my 2000)

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
FRANCE | TOTAL ACTIVA DIESEL 5000 TOTAL ACTIVA DIESEL 7000 TOTAL ACTIVA DIESEL 9000 TOTAL ACTIVA 9000 (6) | 15W40 10W40 5W40 5W30 | CF CF CF CF | B2 B3 B3 specific to Peugeot
Germany Austria Belgium Belorussia Bosnia Bulgaria Cyprus Croatia Denmark Spain Estonia Finland Great Britain Greece Hungary Ireland Italy Latvia Lithuania Luxemburg Macedonia Malta Norway Netherlands Poland Portugal Czech Republic Rumania Russia Slovenia Sweden Switzerland | TOTAL QUARTZ DIESEL 5000 TOTAL QUARTZ DIESEL 7000 TOTAL QUARTZ 9000 TOTAL QUARTZ 9000 (6) | 15W40 10W40 5W40 5W30 | CF CF CF CF | B2 B3 B3 specific to Peugeot
(6) this energy saving oil can only be used with engines designed to receive it (from my 2000)

4 - 2 - AFRICA

Country | ESSO | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Tunisia | ESSO ULTRON DIESEL | 5W40 | CF | B3

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
all countries | TOTAL QUARTZ DIESEL 5000 TOTAL QUARTZ DIESEL 7000 TOTAL QUARTZ 9000 | 15W40 15W50 5W40 | CF CF CF | B2 B3 B3

4 - 3 - SOUTHERN EUROPE

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Turkey | TOTAL QUARTZ DIESEL 5000 TOTAL QUARTZ DIESEL 7000 TOTAL QUARTZ 9000 | 15W40 15W50 5W40 | CF CF CF | B2 B3 B3

4 - 4 - FRENCH OVERSEAS TERRITORIES

Country | ESSO | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
French West Indies Reunion | ESSO UNIFLO DIESEL ESSO ULTRA DIESEL ESSO ULTRON DIESEL | 15W40 10W40 5W40 | CF CF CF | B2 B3 B3

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Caribbean Pacific Polynesia Reunion | TOTAL ACTIVA DIESEL 5000 TOTAL ACTIVA DIESEL 7000 TOTAL ACTIVA DIESEL 7000 TOTAL ACTIVA DIESEL 9000 | 15W40 15W50 10W40 5W40 | CF CF CF CF | B2 B3 B3 B3

4 - 5 - MIDDLE EAST

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Bahrain United Arab Emirates Kuwait Lebanon Oman Qatar Yemen | TOTAL QUARTZ DIESEL 5000 TOTAL QUARTZ DIESEL 7000 TOTAL QUARTZ 9000 | 15W40 15W50 5W40 | CF CF CF | B2 B3 B3

4 - 6 - SOUTH-EAST ASIA

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
China India Indonesia JAPAN Malaysia Singapore Taiwan Thailand Vietnam | TOTAL QUARTZ DIESEL 5000 TOTAL QUARTZ DIESEL 7000 TOTAL QUARTZ DIESEL 7000 TOTAL QUARTZ 9000 | 15W40 15W50 10W40 5W40 | CF CF CF CF | B2 B3 B3 B3

4 - 7 - SOUTH AMERICA

Country | ESSO | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Argentina Bolivia Paraguay Uruguay | ESSO UNIFLO DIESEL ESSO ULTRA DIESEL | 15W40 10W40 | CF CF | B2 B3

Country | TOTAL | grade | API standards | ACEA standards
--- | --- | --- | --- | ---
Argentina Bolivia Brazil Chile Paraguay Uruguay | TOTAL QUARTZ DIESEL 5000 TOTAL QUARTZ DIESEL 7000 TOTAL QUARTZ DIESEL 7000 TOTAL QUARTZ 9000 | 15W40 15W50 10W40 5W40 | CF CF CF CF | B2 B3 B3 B3