C5HG2GF1 - 206

REMOVAL - REFITTING HEATER MATRIX

1 - SPECIAL TOOLS

[1] Hose clamp (-).1512 .

[2] Pliers for spring collar (-).0165 .

2 - REMOVAL

Disconnect the battery .

Remove :

- the fascia
- the heater

Using a pair of pliers, cut the securing tabs (1) .

Using a pair of pliers, cut the securing tabs (2) .

Remove :

- the fastener (3), (4)
- all the heater matrix pipes
- the matrix

3 - REFITTING

Secure all the heater matrix pipes on the heater matrix using nut bolts (4), (5) .

Secure the heater matrix to the air conditioner using bolts (6) .

IMPERATIVE : in the case of replacement of all the heater matrix pipes, securing to the heater matrix is by the tabs (2) and the bolt (4) .