B1FB0SK1 - 206 DV4TD ENGINE

DATA TIGHTENING TORQUE(S) LUBRICATION

1 - DATA

1 - 1 - OIL CAPACITY

engine code | 8HZ -8HX
--- | ---
special features | without
oil capacity with replacement of the oil filter : litre(s) | 3.75
oil capacity without replacement of the oil filter : litre(s) | -
difference between the minimum and the maximum : litre(s) | 1.8
oil filter capacity : litre(s) | 0.4

IMPERATIVE : with the engine stopped ; always check the oil level using the dipstick .

1 - 2 - OIL PRESSURE

WARNING : the values are given in bars, at a temperature of 110 degrees C .

minimum pressure (bars)
engine code | 8HZ - 8HX
--- | ---
special features | without
check 1 at 1000 rpm | 1.3
check 2 at 2000 rpm | 2.3
check 3 at 3000 rpm | 3.3
check 4 at 4000 rpm | 3.5

2 - TIGHTENING TORQUE(S)

Tighten in the order indicated .

reference / description | 8HZ - 8HX
--- | ---
special features | without
oil pump : pre-tightening | 0.5
oil pump : tightening | 1
filter gauze - oil pump | 0.5
filter gauze - cylinder block | 0.5
upper dipstick | 1
exchanger | 1.2
oil filter bracket | 1
drain plug | 1.6
nut for sump | 1
fixing for lubrication pipe - turbocharger | 2.2
fixing for lubrication pipe - cylinder block | 2.2