C--B00F1 - 206

RECOMMENDED PRODUCTS BODYWORK

1 - EXTRUSION MASTICS

applications - data | suffix : | products Part No. | supplier(s)
--- | --- | --- | ---
sealing of panel bonds after welding product which dries in the air and which can be painted | A1 | 9726.68 | TEROSON
GURIT glass adhesive : - complete bi-component kit - complete mono-component kit - cartridge with nozzle | A3 | repair kit : 9799.58 (1) 9798.96 9725.21 | GURIT ESSEX
TOGOCOLL glass adhesive : - complete mono-component kit - cartridge with nozzle | repair kit : 9799.C8 (2) 9799.E0 | SPCA
repair kit rapid version | 9799.57 | GURIT ESSEX
repair kit : - ultra rapid version - rapid version - standard version | repair kit / bonding 9799.E3 (3) 9799.E4 (4) 9799.E5 (5) | TEROSON
additional cartridge : - ultra rapid version - rapid version - standard version | 9726.74 9726.75 9726.76 | TEROSON
(1) = to be used with the BETAGUN gun (2) = to be used with the P 500 gun (3) = to be used with the POWER-LINE gun (4) = to be used with the MULTI-PRESS gun | 9799.F4 9799.C9 9799.E7 9799.E6 | GURIT ESSEX SPCA TEROSON TEROSON
repair kit / hood complete kit : - cartridges/nozzles - primers (2) - applicator pads | 9734.G5 | GURIT ESSEX
sealing of crimpings (mastic in white cartridge) allow to dry for about 1 hour(s) at 20 degrees C before painting | A4 | PU 522 9726.44 TEROSTAT 9101 9734.A7 BETAFILL 9734.C3 | SPCA TEROSON GURIT ESSEX

2 - PREFORMED MASTICS - SOUND PROOFING PADS

applications - data | suffix : | products Part No. | supplier(s)
--- | --- | --- | ---
filling mastic which ensures sealing between components fastened with bolts (wings...) apply to panels protected by primers or paint (round section) | H1 ø = 6 mm H2 ø = 13 mm H3 ø = 20 mm | M110 9725.68 M110 9725.69 | CEPAC RHODORSEAL
(rectangular section) BUTYL mastic preformed for sealing the sun roof and door panels silicon mastic for sealing the sun roof and insert (310 ml) | H4 2 x 20 mm ø 4.5 x 10 m | M110 9725.70 M310 9725.79 R5522 9734.C9
sound proofing pads (self-adhesive) apply to protected panels (paint or primers) | H5 250 x 500 | R99 9725.61 BLACKSON.40 9728.82 SEPTUM 9727.95 | RESTAGRAPH BLACKSON CEPAC

3 - ADHESIVES

applications - data | suffix : | products Part No. | supplier(s)
--- | --- | --- | ---
glass-metal adhesion rear-view mirror door window sill | B1 | 9733.13 9731.10 9735.71 | FRAMET CEPAC
bonding of interior trim (fabrics, carpet, felt) | B2 | 8080 E 9724.51 8090 9724.33 8150 9885.42 C 155 9724.39 SUPER TACK 9728.E4 | 3M CEPAC 3M 3M 3M CEPAC
door panel bonding kit | B3 | 9731.73 | HENKEL
bonding of badge, moulding.. double-sided adhesive | B6 | 9885.97 | 3M
bonding of the rain sensor bonding : third brake light bonding of interior trim (fabrics, carpet, felt) | B7 | 9724.51 9885.41 | TEROSON 3M

4 - GREASES

applications - data | suffix : | products Part No. | supplier(s)
--- | --- | --- | ---
molybdenum bisulfide based multi-purpose lubricant | G5 | ESSO 3106 9735.68 | CEPAC
multi-purpose grease | G6 | ESSO 3106 9735.72
lubricant for sliding the windows in the door seal | G11 | KRYTOK. GPL103 9718.78

5 - PROTECTIVE PRODUCTS

applications - data | suffix : | products Part No. | supplier(s)
--- | --- | --- | ---
under body anti-corrosion protection coating to be applied to panels pre-coated with primer or treated cataphoretically | C1 | CT 9725.74 IP 80 9725.50 protector (PHP) 9734.A3 AG 386 9734.39 8864 9732.99 | TEROSON BLACKSON REVCO SPCA 3M
protection of door surrounds and tailgate frame coating to be applied to panels pre-coated with primer or treated cataphoretically | C2 | TEROSTAT 9101 9734.A7 BLACKSON 165 9725.67 PU 522 9726.45 BETAFILL 9734.C3 | TEROSON BLACKSON SPCA GURIT ESSEX
anti-chip protection coating to be applied to panels pre-coated with primer or treated cataphoretically allow to dry for about 1/2 hour(s) at 20 degrees C before painting | C4 | IP 200 (monocomponent) 9734.48 AG 1124 (bicomponent) 9734.54 REVOTHANE (bicomponent) 9734.A2 | BLACKSON SPCA REVCO
protection of hollow bodies to be sprayed into hollow areas using the appropriate holes | C5 | PROTEX CS39 9740.36 BP 90 9736.07 REVONOX 9734.A0 | SPCA BLACKSON REVCO
polyurethane foam for hollow areas (cartridge) | C6 | BLACKSON 890 9726.13 | BLACKSON
internal protection of the spot welding lines : conducting preparation applied to the internal surface of the panels, before welding | C7 | SOUDOCUIVRE 9739.F1 CEPACUIVRE 9739.F2 | REVCO GURIT CEPAC
re-zincing panels (using the re-zincing unit) | C8 | (5)

(5) Special order :

- electro-zinc plating unit (DALIC) Part No. 9769.47
- zinc consumables pack : Part No. 9769.48

(5) Special order :

- electro-zinc plating unit (SELECTRON) Part No. 9913.21
- zinc consumables pack : Part No. 9913.22

6 - REPAIR OF COMPOSITE MATERIALS (SMC)

applications - data | suffix : | products Part No. | supplier(s)
--- | --- | --- | ---
repair of slight cracks, scratches, adhesive layer polyester mastic filled with V.11 glass fibre | K1 | GLASSFIBER 9726.83 | PEUGEOT
225 g/m2 glass fibre mat | K2 | CEPACTOL 9733.08 | CEPAC