C4AH1VF1 - 206 CABRIOLET

REPLACEMENT REAR WING INNER PANEL REAR PILLAR

IMPERATIVE : THIS VEHICLE HAS BEEN DESIGNED USING THE MIG BRAZE WELDING TECHNIQUE ; when the structure is repaired, all the connections concerned must be welded using the same procedure ; any other technique is prohibited .

WARNING : all the scoured areas must be protected by the approved electrolytic re-zincing process .

IMPERATIVE : observe elementary health and safety rules (wearing of filter mask for organic fumes - work in a ventilated area) .

1 - COMPLEMENTARY OPERATION(S)

Replacement :

- REAR WING ASSEMBLY
- rear pillar stiffener
- OUTER SILL
- tail panel assembly

2 - IDENTIFICATION OF REPLACEMENT PARTS

(1) Rear wing inner panel assembly .

(2) Rear pillar .

(3) Passenger compartment rear partition strengthener .

(4) Rear seat belt strap guide bracket .

3 - PART(S) REQUIRED TO CARRY OUT THE OPERATION

(1) Rear wing inner panel assembly .

(2) Rear pillar .

(3) Passenger compartment rear partition strengthener .

(4) Rear seat belt strap guide bracket .

4 - PREPARATION OF THE NEW PART

5 - CUTTING OUT

6 - RELEASING

7 - ADJUSTMENT

8 - WELDING

9 - PROTECTION