C5GG24F1 - 206

REMOVAL - REFITTING REAR SEAT

1 - REMOVAL : REAR SEAT CUSHION

Release the hinges (1) following the direction of the arrows .

2 - REMOVAL : BACKREST

Remove the fasteners (2) - (3) .

NOTE : it is necessary to remove the 2/3 backrest before removing the 1/3 backrest .

3 - REFITTING

Proceed in the reverse order to removal .

4 - TIGHTENING TORQUE(S)

Tighten the bolts (2) to 2,3 daN.m .

Tighten the bolts (3) to 2,3 daN.m .