C4CH1XF1 - 206 CABRIOLET

REPLACEMENT OUTER SILL

IMPERATIVE : THIS VEHICLE HAS BEEN DESIGNED USING THE MIG BRAZING PROCESS TECHNIQUE ; when the structure is repaired, all the connections concerned must be welded using the same procedure ; any other technique is prohibited .

WARNING : all the scoured areas must be protected by the approved electrolytic re-zincing process .

IMPERATIVE : observe elementary health and safety rules (wearing of filter mask for organic fumes - work in a ventilated area) .

1 - COMPLEMENTARY OPERATION(S)

Replacement :

- DOOR

Removal - refitting :

- front, rear mud guard
- front wing
- door aperture seal
- FRONT SEAT
- REAR SEAT CUSHION
- REAR SEAT BACKREST

Remove-refit trim :

- front pillar
- centre pillar
- part front floor
- part rear floor

Detach the electrical harnesses .

2 - IDENTIFICATION OF REPLACEMENT PARTS

Outer sill (1) .

3 - PART(S) REQUIRED TO CARRY OUT THE OPERATION

Outer sill (1) .

4 - PREPARATION OF THE NEW PART

5 - CUTTING OUT

6 - SEPARATING

7 - ADJUSTMENT

8 - WELDING

9 - SEALING

10 - PROTECTION