B1FI02V1 - 206

ENGINE CAPACITIES

106 - petrol
| capacities in litres
--- | ---
engine type | without filter | with filter
TU (not TU5J4) gravity draining | 2,90 | 3,20
TU (not TU5J4) suction draining | - | 3,25
TU5J4 gravity draining | 2,90 | 3,20
TU5J4 suction draining | 3,10 | 3,40
imperative : in every case, check the level and top-up if necessary

106 - Diesel
- | capacities in litres
--- | ---
engine type | with filter
TUD3 | 3,50
TUD5 | 4,50
imperative : in every case, check the level and top-up if necessary

206 - petrol
engines | engines | capacities in litres | capacities in litres
--- | --- | --- | ---
engine code | engine type | with filter | between min and max dipstick
HFX - HFY HFZ - K6C - KFW KFX - NFZ | TU (not TU5JP4 ) gravity draining | 3,00 | 1,50
HFX - HFY HFZ - K6C - KFW KFX - NFZ | TU (not TU5JP4) suction draining | 3,25 | 1,50
N6A - NFU | TU5JP4 gravity draining / suction draining | 3,25 | 1,50
RFN - RFR | EW10J4 | 4,25 | 1,70
imperative : in every case, check the level and top-up if necessary

206 - diesel
engines | engines | capacities in litres | capacities in litres
--- | --- | --- | ---
engine code | engine type | with filter | between min and max dipstick
WJY - WJZ | DW8 | 4,75 | 1,60
RHY | DW10TD | 4,50 | 1,40
imperative : in every case, check the level and top-up if necessary

306 - petrol
| capacities in litres
--- | ---
engine type | without filter | with filter
XU10J4R air con. | 3,95 | 4,25
XU10J4R no air conditioning | 4,45 | 4,75
XU10J2C air con. | 3,95 | 4,25
XU10J2C no air conditioning | 4,20 | 4,50
XU7JP air con. | 3,95 | 4,25
XU7JP no air conditioning | 4,45 | 4,75
XU10J4D air con. | 3,95 | 4,25
XU10J4D no air conditioning | 4,20 | 4,50
XU7JP4 air con. (dipstick handle - colour : orange) | 3,95 | 4,25
XU7JP4 air con. (dipstick handle - colour : yellow) | - | 4,50
XU7JP4 no air conditioning (dipstick handle - colour : orange) | 4,45 | 4,75
XU7JP4 no air conditioning (dipstick handle - colour : yellow) | - | 5,00
XU10J4RS | - | 4,25
TU gravity draining | 2,90 | 3,20
TU suction draining | - | 3,25
imperative : in every case, check the level and top-up if necessary

306 - Diesel
- | capacities in litres
--- | ---
engine type | with filter
XUD9A air con. | 4,00
XUD9A no air conditioning | 4,50
XUD9TE air con. | 4,00
XUD9TE no air conditioning | 4,50
XUD7 air con. | 4,00
XUD7 no air conditioning | 4,50
DW8 air con. | 4,50
DW8 no air conditioning | 4,75
DW10TD air con. | 4,25
DW10TD no air conditioning | 4,50
imperative : in every case, check the level and top-up if necessary

406 - petrol
- | capacities in litres
--- | ---
engine type | with filter
XU5JP/XU7JP air con. | 4,25
XU5JP/XU7JP steel sump | 4,75
XU7JP4 air con. (dipstick handle - colour : orange) | 4,25
XU7JP4 air con. (dipstick handle - colour : yellow) | 4,50
XU7JP4 no air conditioning (dipstick handle - colour : orange) | 4,75
XU7JP4 no air conditioning (dipstick handle - colour : yellow) | 5,00
XU10J4R air con. | 4,25
XU10J4R no air conditioning | 4,75
XU10J2CTE air con. | 4,50
XU10J2CTE no air conditioning | 4,75
ES9 suction draining | 5,25
ES9 gravity draining | 4,75
XU7JB air con. | 4,50
XU7JB no air conditioning | 5,00
EW7J4 | 4,25
EW10J4 | 4,25
EW12J4 | 4,25
imperative : in every case, check the level and top-up if necessary

406 - Diesel
- | capacities in litres
--- | ---
engine type | with filter
XUD9BTF/XUD9TF air con. | 4,00
XUD9BTF/XUD9TF no air conditioning | 4,50
XUD11BTE air con. | 4,75
XUD11BTE no air conditioning | 5,25
XUD9SD air con. | 4,25
XUD9SD no air conditioning | 4,00
DW10ATED | 4,50
DW10TD | 4,50
DW12TED4 | 4,75
imperative : in every case, check the level and top-up if necessary

806 - petrol
- | capacities in litres
--- | ---
engine type | with filter
XU10J2C air con. | 4,50
XU10J2C no air conditioning | 4,75
XU10J2CTE air con. | 4,50
XU10J2CTE no air conditioning | 4,75
XU7JP air con. | 4,25
XU7JP no air conditioning | 4,75
XU10J4R | 4,25
EW10J4 | 4,25
imperative : in every case, check the level and top-up if necessary

806 - Diesel
- | capacities in litres
--- | ---
engine type | with filter
XUD9TF air con. | 4,00
XUD9TF no air conditioning | 4,25
XUD9BTF air con. | 4,00
XUD9BTF no air conditioning | 4,25
XUD11BTE air con. | 4,25
XUD11BTE no air conditioning | 4,75
DW10ATED | 4,50
DW10ATED4 | 4,75
imperative : in every case, check the level and top-up if necessary