C5KG0EF1 - 206

REMOVAL - REFITTING ELECTRIC SUN ROOF OPENING MECHANISM

1 - REMOVAL

Remove :

- the headlining
- the interior tailgate frame
- the sun roof

Manually open the moving panel 200 mm .

Remove the electric motor (1) .

Remove the drive pins (2) .

Remove the fasteners (3) .

Remove the opening mechanism .

2 - REFITTING

IMPERATIVE : check : the coupling of the motor to its mechanism ; the clipping of the cable sleeves ; that the condition of the seals on the frame is perfect .

Proceed in the reverse order to removal .