C4BH32F1 - 206 CABRIOLET

REPLACEMENT TAIL PANEL ASSEMBLY

IMPERATIVE : THIS VEHICLE HAS BEEN DESIGNED USING THE MIG BRAZING PROCESS TECHNIQUE ; when the structure is repaired, all the connections concerned must be welded using the same procedure ; any other technique is prohibited .

WARNING : all the scoured areas must be protected by the approved electrolytic re-zincing process .

IMPERATIVE : observe elementary health and safety rules (wearing of filter mask for organic fumes - work in a ventilated area) .

1 - SPECIAL FEATURE

On adjustment of the rear wing assembly, use either the jig tools or mechanical or electronic measuring equipment .

2 - COMPLEMENTARY OPERATION(S)

Replacement :

- REAR BUMPER

Removal - refitting :

- tail lamps
- tailgate aperture seal
- boot carpet
- DOOR STRIKER

Remove-refit trim :

- rear panel

Detach :

- the electrical harnesses

3 - IDENTIFICATION OF REPLACEMENT PARTS

Tail panel assembly .

4 - REPLACEMENT PART COMPOSITION

(1) Tailgate striker fixing stiffener .

(2) Tail panel inner panel .

(3) Rear panel .

(4) Rear bumper upper support .

5 - PART(S) REQUIRED TO CARRY OUT THE OPERATION

Tail panel assembly .

6 - PREPARATION OF THE NEW PART

7 - CUTTING OUT

8 - SEPARATING

9 - ADJUSTMENT

10 - WELDING

11 - SEALING

12 - PROTECTION