C5CG0TF1 - 206

REMOVAL - REFITTING FRONT DOOR OPENING MECHANISM

1 - REMOVAL

Raise the glass .

Remove :

- the door trim panel
- the seal

Unclip the connection rod (1) on the outer handle .

Remove the interior handle (2) by pulling the handle towards the hinges .

Release the clip (3) .

Remove the fasteners (4) .

Release : The electrical connection (5) .

Unclip this connection from the control unit .

Remove the mechanism assembly (A) by turning it to detach the pin from the lock .

Pass the assembly through the opening (B) .

2 - REFITTING

WARNING : connect the electrical harness of the electrical control unit after it has been refitted (secure the connection by pressing) (according to specification) .

IMPERATIVE : fit new seals, which must be assembled without folds and tears ; absolute cleanness of the contact face on the vehicle is necessary, pass a small roller over the pre-bonded sections of the sheet .

IMPERATIVE : these recommendations are essential to prevent possible entry of water, dust or noise .

Proceed in the reverse order to removal .