B2BB0QK1 - 206 BE4 GEARBOX

PRESENTATION TOOLING GEARBOX

1 - SPECIAL TOOLS

reference | description | reference | reference
--- | --- | --- | ---
[1] | universal extractor bridge piece | FACOM U53 K2 | 4108 - T
[2] | universal separator tool | FACOM U53 T2 | 4108 - T

reference | description | reference | reference
--- | --- | --- | ---
[3] | drift for extracting and fitting the input shaft bearing | (-).0317 - A (-).0317 - AR | 7101 - TA 0317 - AR
[4] | input shaft front and rear bearing and output shaft rear bearing fitting drift | (-).0317 - F | 7101 - TF
[5] | 6th gear bearing removal drift (output shaft) | (-).0317 - EZ | 7101 - TE

reference | description | reference | reference
--- | --- | --- | ---
[6] | input shaft nut removal-refitting sleeve | (-).0317 - AN | 317 - AN

reference | description | reference | reference
--- | --- | --- | ---
[7] | 5th gear extractor claw | (-).0331 - F | 0331 - F
[8] | extractor | (-).0331 - A | 5703 - T

reference | description | reference | reference
--- | --- | --- | ---
[9] | fitting drift for final drive right-hand output oil seal | (-).0317 - U | 7114 - TX
[10] | fitting drift for final drive left-hand output oil seal | (-).0317 - T | 7114 - TW

reference | description | reference | reference
--- | --- | --- | ---
[11] | dial gauge support assembly |
[11a] | dial gauge support rod | (-).0317 - AP | 0317 - AP
[11b] | dial gauge support | (-).0330 - V2 | 5708 - TV2
[11c] | dial gauge support rod | (-).0330 - V3 | 5708 - TV3

reference | description | reference | reference
--- | --- | --- | ---
[12] | dial gauge | (-).1504 | 2437 - T

reference | description | reference | reference
--- | --- | --- | ---
[13] | slide hammer assembly |
[13a] | slide hammer | (-).0316 - A | 1671 - T
[13b] | adaptor | (-).0317 - V | 7113 - TX

reference | description | reference | reference
--- | --- | --- | ---
[14] | differential bearing fitting tube | (-).0317 - D | 701 - TD
[15] | thrust button | (-).0317 - JZ | 4508 - TI

reference | description | reference | reference
--- | --- | --- | ---
[16] | 5th speed hub extractor | (-).0317 - Y | 7116 - E

reference | description | reference | reference
--- | --- | --- | ---
[17] [17a] [17b] | pin fitting tool | (-).0317 - AM | 8013 - T.AM

reference | description | reference | reference
--- | --- | --- | ---
[18] [18a] [18b] | gear lever pin extractor | (-).0317 - AL | 8013 - T.AL

reference | description | reference | reference
--- | --- | --- | ---
[19] | fitting and removal drift for 6th gear bearing outer race in the 5th/6th housing | (-).0317 - AE | -
[20] | thrust button | (-).0317 - AF | -
[21] | input and output shaft bearing fitting drift | (-).0317 - AH | -

reference | description | reference | reference
--- | --- | --- | ---
[22] | thrust washer under pinion | (-).0317 - AG | -

reference | description | reference | reference
--- | --- | --- | ---
[23] | input shaft oil seal fitting drift | (-).0317 - W | -
[24] | basic shim | (-).0317 - X | -
[25] | sling | (-).0328 | -

reference | description | reference | reference
--- | --- | --- | ---
[26] | tool for unclipping 10 dia. ball joints | (-).0216-G1 | -
[27] | tool for unclipping 13 dia. ball joints | (-).0216-G2 | -

reference | description | reference | reference
--- | --- | --- | ---
[28] | fitting drift for final drive right-hand output oil seal | (-).0317-U | -
[29] | fitting drift for final drive left-hand output oil seal | (-).0317-T | -

reference | description | reference | reference
--- | --- | --- | ---
[30] | gearbox pin removal-refitting socket | (-).0317-AB | -

reference | description | reference | reference
--- | --- | --- | ---
[31] | final drive right-hand output oil seal fitting drift (four wheel drive) | 7116 - TB | (-).0326 - E
[32] | protector | 7116 - TC | (-).0326 - F

reference | description | reference | reference
--- | --- | --- | ---
[33] | depth gauge | FACOM 811 | FACOM 811

reference | description | reference | reference
--- | --- | --- | ---
[34] | three legged extractor | FACOM U20 | -

reference | description | reference | reference
--- | --- | --- | ---
[35] | locking tool | (-).0526 - J | 70902 - K