B3FG1MK1 - 206

REMOVAL - REFITTING LOAD SENSITIVE COMPENSATOR

1 - REMOVAL

Remove the filter from the brake fluid reservoir .

DRAIN THE BRAKE FLUID RESERVOIR USING A CLEAN SYRINGE .

Move aside the brake pipes (1) .

Block the openings in the pipes and the compensator .

Slacken the bolt (2) .

Remove :

- the bolt (3)
- the compensator (4)
- the bolt (5)
- the spring (6)

2 - REFITTING

Parts Division supplies the compensator with a shim (7) used in production .

Do not use this shim for adjusting the brake pressure during Service operations .

Remove the block .

Proceed in the reverse order to removal .

Ensure that the spring (6) is correctly positioned on the spacer (8) .

Coat the bolt (5) with threadlock LOCTITE .

Tighten the bolt (5) to 2 da.Nm .

Position :

- the spring (6) in the compensator lever
- the compensator on its bracket

In order to adjust the clearance at the centralising dowel pin (9) apply force in the direction of the arrow .

Coat the bolt (3) with threadlock LOCTITE .

Tighten the bolt (3) to 1.75 da.Nm .

Tighten the brake pipes to 1.5 daN.m .

Tighten the bolt (2) to 1.3 da.Nm .

BLEED THE BRAKES .

IMPERATIVE : ADJUST THE LOAD SENSITIVE COMPENSATOR .