C5JH06F1 - 206

REPLACEMENT STEERING LOCK

1 - REMOVAL

Disconnect the battery .

Remove :

- the column half cowls
- the fascia lower trim

Disconnect the connectors .

Release the analogue module .

Place the steering wheel in the lowest position .

Remove : The securing bolt (1) .

Release the ignition switch supply harnesses .

Insert the key (2) in the ignition switch .

Place the key in the intermediate position, between positions (A) and (M) .

Press at points (3) to release the ignition switch .

Remove the ignition switch .

2 - REFITTING

Proceed in the reverse order to removal .