C4BG20F1 - 206 CABRIOLET

ADJUSTMENT BOOT UPPER COVER LOCKING MECHANISM

IMMOBILISE THE BOOT UPPER COVER .

Unscrew the mounting nuts (1) .

Retighten the mounting nuts (1) by hand .

TIGHTEN THE RELIEF SCREW .

Unfold the tray (luggage cover screen .

Switch on the ignition .

Release the two front locking systems on the roof .

Remove the immobilisation tool from the cover .

Close the boot upper cover by pressing the roof control switch .

Open the luggage compartment .

Visually check the position of the hook (2). it should be located in the centre of the locking mechanism hinge pin (3) .

Tighten the nuts (1) to 1 ± 0.1 da.Nm .

Close the boot again .

Carry out one cycle of operation .

CHECK THE FITS AND CLEARANCES .

NOTE : if the values are not correct, replace the rubber of the slots and of the base pipes (4) then repeat the adjustment operation .