C4BH30F1 - 206 CABRIOLET

REPLACEMENT OF THE C POST INNER PANEL

IMPERATIVE : this vehicle has been designed using the mig cupro-soldering technique ; when the structure is repaired, all the connections concerned must be welded using the same procedure ; any other technique is prohibited .

WARNING : all the scoured areas must be protected by the approved electrolytic re-zincing process .

IMPERATIVE : observe elementary health and safety rules (wearing of filter mask for organic fumes - work in a ventilated area) .

1 - COMPLEMENTARY OPERATION(S)

Replacement :

- REAR WING

2 - IDENTIFICATION OF REPLACEMENT PARTS

"C" post inner panel .

3 - PART(S) REQUIRED TO CARRY OUT THE OPERATION

"C" post inner panel .

4 - PREPARATION OF THE NEW PART

5 - CUTTING OUT

6 - RELEASING

7 - ADJUSTMENT

8 - WELDING

9 - SEALING

10 - PROTECTION