C5IG13F1 - 206 CABRIOLET

REMOVAL - REFITTING ROOF OPENING/CLOSING CONTROL SWITCH

1 - REMOVAL

Using a spatula remove the switch bracket (1) .

Disconnect the switch .

Unclip the switch (2) from the bracket (1) at (A) - (B) .

Remove the switch (2) .

2 - REFITTING

IMPERATIVE : ensure that the switch (2) is correctly clipped onto the bracket (1) .

Proceed in the reverse order to removal .

Perform several tests of operation .