B1GG12K1 - 206 D4D ENGINE MERCOSUR

REMOVAL - REFITTING COOLANT PUMP

1 - REMOVAL

Place the vehicle on a two-post ramp .

Remove the stone shield panel .

Drain the cooling system .

Remove :

- the ancillary drive belt
- the timing belt and its dynamic tensioner

Partially remove the air conditioning compressor (1) .

Move aside the air conditioning compressor and place it on the front surface .

Remove the support (2) .

Remove the coolant pump (3) .

2 - REFITTING

WARNING : clean the joint faces with an approved descaling product ; do not use sharp or abrasive tools ; the joint faces must not have any trace of knocks or scores .

place a bead of sealant E10 on the coolant pump joint surface .

Fit :

- the coolant pump : tighten the bolts to 2.2 daN.m
- the timing belt and its dynamic tensioner
- the ancillary drive belt

Continue the fitting operations in the reverse order to removal .

Fill and bleed the cooling system .