B2CG76K1 - 206 AL4 AUTOMATIC GEARBOX

REMOVAL - REFITTING AUTOMATIC GEARBOX INPUT SPEED SENSOR (AL4)

1 - REMOVAL

NOTE : do not drain the gearbox .

Disconnect the battery .

Remove :

- the ECU cover
- the connector of the engine ecu
- the air cleaner housing
- the air hose
- the battery
- the battery container

Remove the 2 bolts (1) (Mounting of the modular connector on the gearbox) .

Disconnect the modular connector (2) .

Extract the 3-way connector (4) from the modular connector (2) .

NOTE : gearbox input speed sensor .

Remove :

- the front left-hand wheel
- the sensor harness (5)
- the bolt (6)
- gearbox input speed sensor (5)

2 - REFITTING

Replace the sensor o ring (5) .

Fit :

- gearbox input speed sensor (5)
- the bolt (6) (tightening torque 1 da.Nm)
- the sensor harness (5)
- the yellow 3-way connector (4) in the modular connector (2)
- the 2 bolts (1) (tightening torque 1 da.Nm)

Reconnect the modular connector (2) .

Fit :

- the front left-hand wheel
- the battery container
- the battery
- the air cleaner housing
- the air hose
- the connector of the engine ecu
- the ECU cover

Connect the battery .