B1HG2BK1 - 206 EW10J4 ENGINE DW8 ENGINE TU ENGINE

REMOVAL - REFITTING FUEL TANK

1 - SPECIAL TOOLS

EW10J4 ENGINE TU ENGINE

[1] Pipe with adapter for valve SHRADER (-).0141-T1 .

ALL MODELS

2 - REMOVAL

EW10J4 ENGINE TU ENGINE

Drop the pressure in the supply pipe by connecting the end of the equipment [1] to the engine fuel supply circuit .

ALL MODELS

Empty the tank using draining equipment .

Place the vehicle on a lift with rear wheels suspended .

Remove :

- the right hand rear wheel
- the mud shield

Remove : The securing bolts (1) (Fuel filler neck) .

Remove the intermediate silencer .

Remove the metal heat shield (2) .

Unclip the hand brake cables from the tank .

Remove the tank securing bolts (3) .

Lower the tank without removing it .

Disconnect :

- the pipes connected to the tank and to the filler neck
- the fuel gauge connector

Remove : Tank and filler neck assembly .

3 - REFITTING

Re-assemble in the reverse order to dismantling .