C5IG10F1 - 206 CABRIOLET

REMOVAL - REFITTING RETRACTABLE ROOF ASSEMBLY

1 - TOOLS

[1] cross beam (-).0102-D .

[2] Set of 4 straps (-).0916-B .

[3] lifting hooks (-).0102-J / (-).0102-G .

[4] Set of 4 shackles (-).0916-C .

[5] Mobile hydraulic crane .

2 - REMOVAL

REMOVE THE BOOT ASSEMBLY .

REMOVE THE SCREEN (LUGGAGE COVER) .

Disconnect the ecu (1) connector (2) .

Unclip and disconnect the rear screen/passenger compartment/end of travel switches harnesses (3) .

Retain the harnesses on the metal frame prior to handling .

Remove the fasteners (4) .

REMOVE THE MOVING REAR SHELF .

Refit the roof supports temporarily .

Fold the roof in the boot .

NOTE : store the boot upper cover struts in the folded roof free space (take the necessary precautions) .

Remove the fasteners (5) .

WARNING : do not touch the frame centring pins (6) .

Attach adhesive tape to the roof at (A) to protect the flange .

Raise the rear moving shelf mechanism (B) .

Position the tools [1] - [2] - [3] - [4] - [5] .

Raise the folding roof assembly .

Remove the roof assembly taking care to protect the rear screen in contact .

3 - REFITTING

Position the roof assembly on the body using pins (6) .

Detach and remove the tools [1] - [2] - [3] - [4] - [5] .

Fit the fasteners (5) .

REFIT THE MOVING SHELF ON ITS MECHANISM THEN PLACE IT VERTICALLY AGAINST THE PARTITION .

Detach the protective tape (A) .

Close the folding roof manually .

Check that there is no roof operating stress .

Remove the roof supports .

Fit the fasteners (4) .

Tighten :

- the fastenings (4) to 1 ± 0.2 da.Nm
- the fastenings (5) to 2,5 ± 0,2 da.Nm

REFIT THE BOOT ASSEMBLY .

Clip, clamp and connect the connectors (1) - (3) and the harnesses .

REFIT THE SCREEN (LUGGAGE COVER) .

Carry out a roof/boot assembly operation check .

CHECK THE SEALING OF THE VEHICLE .