B3FG23K1 - 206

REMOVAL - REFITTING FRONT BRAKE CALIPERS BOSCH

1 - REMOVAL

Remove the wheel .

REMOVE THE BRAKE PADS .

Disconnect : The brake hose to the rigid pipe .

Recover the U clip (1) .

Plug the brake pipe .

Remove the brake hose .

Remove :

- the bolts (2) of the caliper bracket
- the caliper + bracket assembly

2 - REFITTING

Refit the caliper with its bracket .

Fit 2 new bolts (2) (coated with threadlock)) .

Tighten the bolts (2) to 10.5 daN.m .

Fit :

- the brake hose to the caliper
- tightening torque 1.5 da.Nm

Fit :

- the brake hose to the rigid pipe
- tightening torque 1.6 da.Nm

WARNING : take care not the twist the brake hose .

Bleed the brakes .

FIT THE BRAKE PADS .

Fit the wheel .

Tighten the wheel bolts : 8.5 da.Nm .

WARNING : check that the brake hose does not touch the wheel when it is at full lock; if it does, refit the brake hose .