B3FG1HK1 - 206

REMOVAL - REFITTING STOP LAMP SWITCH

1 - REMOVAL

Disconnect the connector (1) .

Remove the switch by pulling it .

2 - REFITTING

Press the brake pedal by hand .

Insert the switch fully into its bracket .

Push the brake pedal to its stop by hand .

The switch should return with the pedal and so be adjusted .

Re-connect the connector (1) .

Switch on the ignition .

Check the lighting of the brake lights .